|  |  |  |
| --- | --- | --- |
|  | Standby RSG Ltd.19 Hollies Business Park, Hollies Park Road, Cannock, Staffordshire WS11 1DB.Tel: 01543 438800 Fax: 01543 438801 Email: info@standbyrsg.co.uk Web: [www.standbyrsg.co.uk](http://www.standbyrsg.co.uk/) | This drawing and its contents are the property of Standby RSG Ltd. All rights in respect of patents, designs and copyrights are reserved. |
| **Universal Multi-Way Switch Unit Specification Sheet - MCS-32** 16 Button Handset Plus UNI-HAP (MCS-T17) |
| ***Please Note:****The 16-way Handset Plus is available with and without* PTT *(Push To Talk). Push to Talk is operated by a switch on the right hand side of the unit. Please ensure that you tick the appropriate box below.*L *= Latching* M *= Momentary, please tick the box next to the appropriate key number if required.**The key colour is created by the LED shining behind the key, please specify the colour required.**Keep words as short as possible and abbreviate long words, if an abbreviation is not stated we will insert a standard abbreviation.*Push to Talk Operating Switch (Optional) |
| Please complete this sheet and return it to Standby RSG Ltd. Orders will not be processed until a signed copy is returned. |
| Customer: | Contact: | Signature: |
| Tel: | Fax: | Email: | Date: |

HW-C-10453-A \_22.06.15



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Switch No. | Legend (eg Front Spots) | Colour | L | M |
| 1 |  |  |  |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |
| 5 |  |  |  |  |
| 6 |  |  |  |  |
| 7 |  |  |  |  |
| 8 |  |  |  |  |
| 9 |  |  |  |  |
| 10 |  |  |  |  |
| 11 |  |  |  |  |
| 12 |  |  |  |  |
| 13 |  |  |  |  |
| 14 |  |  |  |  |
| 15 |  |  |  |  |
| 16 |  |  |  |  |

|  |  |
| --- | --- |
| I DO require PTT (Push to Talk) |  |
| I DO NOT require PTT (Push to Talk) |  |