|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Standby RSG Ltd.  19 Hollies Business Park, Hollies Park Road, Cannock, Staffordshire WS11 1DB.  Tel: 01543 438800 Fax: 01543 438801 Email: [info@standbyrsg.co.uk](mailto:info@standbyrsg.co.uk) Web: [www.standbyrsg.co.uk](http://www.standbyrsg.co.uk/) | | | | | | This drawing and its contents are the property of Standby RSG Ltd. All rights in respect of patents, designs and copyrights are reserved. |
| **Universal Multi-Way Switch Unit Specification Sheet - MCS-32** 16 Button Handset Plus UNI-HAP (MCS-T17) | | | | | | | |
| ***Please Note:***  *The 16-way Handset Plus is available with and without* PTT *(Push To Talk). Push to Talk is operated by a switch on the right hand side of the unit. Please ensure that you tick the appropriate box below.*  L *= Latching* M *= Momentary, please tick the box next to the appropriate key number if required.*  *The key colour is created by the LED shining behind the key, please specify the colour required.*  *Keep words as short as possible and abbreviate long words, if an abbreviation is not stated we will insert a standard abbreviation.*  Push to Talk Operating Switch (Optional) | | | | | | | |
| Please complete this sheet and return it to Standby RSG Ltd. Orders will not be processed until a signed copy is returned. | | | | | | | |
| Customer: | | | Contact: | | Signature: | | |
| Tel: | | Fax: | | Email: | | Date: | |

HW-C-10453-A \_22.06.15



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Switch No. | Legend (eg Front Spots) | Colour | L | M |
| 1 |  |  |  |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |
| 5 |  |  |  |  |
| 6 |  |  |  |  |
| 7 |  |  |  |  |
| 8 |  |  |  |  |
| 9 |  |  |  |  |
| 10 |  |  |  |  |
| 11 |  |  |  |  |
| 12 |  |  |  |  |
| 13 |  |  |  |  |
| 14 |  |  |  |  |
| 15 |  |  |  |  |
| 16 |  |  |  |  |

|  |  |
| --- | --- |
| I DO require PTT (Push to Talk) |  |
| I DO NOT require PTT (Push to Talk) |  |